The selected vendor shall provide full, prompt, accurate, and expert product/services to UNFPA in accordance with the UN policies, procedures, and guidelines.

Please place a tick if the product meets the technical requirements mentioned below:

|  |  |  |
| --- | --- | --- |
| **Specifications** | **Vendor Response (Yes/No)** | **Comments** |
| **Laptop** |
| 14th Gen Intel Mobile Core i7 or Intel® Core™ Ultra Processor 7 or equivalent |   |   |
| At least Four-Core Processor with at least 4.0 GHz speed and at least 12MB cache |   |   |
| At least 16GB DDR4 or DDR5 Memory |   |   |
| At least 512GB Solid State Drive |   |   |
|  Dual-Band (or better) Wireless 802.11ax |   |   |
| At least 1 USB-C Thunderbolt 4.0 port |   |   |
| At least 1 USB-A version 3.2 (Gen 1 or above) port |   |   |
| 1 Audio combo port |   |   |
| 1 HDMI 2.0 (or later) port |   |   |
| Security lock Slot |   |   |
| Touch Screen 13/14" FHD (1920 x 1080) Anti-Glare |   |   |
| Integrated HD Graphics |   |   |
| At least 40Wh Lithium-Ion battery |   |   |
| Built-in English Keyboard |   |   |
| Touch Fingerprint Reader (preferable but not required) |   |   |
| At least 720p resolution webcam |   |   |
| Speaker and noise cancelling digital array microphone |   |   |
| Metal alloy body (for protection while traveling) |   |   |
| AC Adapter with power cord compatible with Fiji socket |   |   |
| Preloaded Windows 11 Professional 64bit |   |   |
| USB-C Docking station (with HDMI and DisplayPort) |   |   |
| Carrying bag for laptop (backpack preferred)  |   |   |
| External Wireless Mouse and Keyboard |   |   |
| Three years battery warranty |   |   |
| At least four years warranty, including accidental damage to the laptop |   |   |
| Next business day onsite service warranty |   |   |
| Compliance and Standards:  ENERGY STAR and TCO Certified laptop |   |   |
| **Monitor** |
| Viewable Size 68.59 cm (27.0 Inches) |   |   |
| Resolution 1920 x 1080 at 60Hz |   |   |
| Contrast Ratio 1000: 1 (typical) |   |   |
| Pixel Per Inch (PPI): 82 |   |   |
| Contrast Ratio 1000: 1 (typical) |   |   |
| Aspect Ratio (16:9) |   |   |
| Backlight Technology LED |   |   |
| Brightness 300 cd/m2 (typical) |   |   |
| 1 x DisplayPort version 1.2 |   |   |
| 1 x HDMI port version 1.4 |   |   |
| 1 x VGA port (preferable but not required) |   |   |
| 1 x USB 3.2 Gen1 Type-B or Type-C upstream |   |   |
| 4 x USB 3.2 Gen1 Type-A or Type-C downstream |   |   |
| Height-adjustable stand |   |   |
| Tilt-adjustable (-5° to 21°) |   |   |
| Swivel – adjustable (-45° to 45°) |   |   |
| 3 years Next business day onsite service warranty   |   |   |
| Power cord compatible with Fiji socket |   |   |
| Compliant Standards ENERGY STAR certified |   |   |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Name, title and signature | Date and place |